# APSystems_devices

# APsystems device coverage

The following APSystems devices are covered :

Inverter Model | Firmware version | Configuration
--- | --- | ---
EZ1 | ≥ 1.7.0 | Continuous local mode

# Continuous local mode for your micro-inverter

## Design

Permanent local mode is a setup configuration of your micro-inverter that allow REST API calls from the local network to the inverter.

Here is the high level network setup :

## Inverter setup

Here is a summary of the expected configuration of each and every inverter to reach. Please refer to official manufacturer user manual for the detailed setup.

Direct-connect device page | Direct-connect device settings | Setting local mode for Continuous local mode
--- | --- | ---