# Antares new features v9.2

    library(antaresEditObject)

This article will present the new features in line with Antares v9.2 (cf Antares Simulator)

## Create new study v9.2

    dir_path <- tempdir()
    suppressWarnings(
      createStudy(path = dir_path,
                study_name = "test920",
                antares_version = "9.2")
    )

For Antares Simulator, format version is now “9.2”. For packages, we make the adjustment and we keep “920”.

Check version of my current study :

    current_study_opts <- simOptions()
    current_study_opts$antaresVersion
    #> [1] 920

Some minor changes to the creation of the study.

Initializes the study by updating the `generaldata.ini` file :

- the value of the `shedding-policy` parameter is changed to “accurate shave peaks”
- a new “compatibility” section is created with parameter `hydro-pmax` = “daily”

## Create area

We just need create areas to create st-storages.

    createArea(name = "fr")
    createArea(name = "it")

A new parameter `overflow spilled cost difference` in `hydro.ini` file (input/hydro/hydro.ini) is initiated (default value = 1).

## Short term storage

We can create new clusters, st-storage (from v8.6), with function `createClusterST()`. You can see function documentation with `?createClusterST`.

By default you can call function only with two parameters (`area`, `cluster_name`).

Clusters are created with default properties and time series.

### Dynamic group names

Default `group` is still “Other1” and now you can create/edit your own group name (only for version study >= 9.2).

    # creation
    createClusterST(area = "fr",
                    cluster_name = "test_storage",
                    group = "my_own_group")

    createClusterST(area = "it",
                    cluster_name = "test_storage",
                    group = "my_own_group_again")

    # edit group of existing st-storage cluster
    editClusterST(area = "fr",
                  cluster_name = "test_storage",
                  group = "my_own_group_Pondage")

    # read cluster properties
    tab <- readClusterSTDesc()
    rmarkdown::paged_table(tab)

### New properties

you can create or edit new clusters with new properties (see doc `?createClusterST`).

    # new properties (default values)
    rmarkdown::paged_table(as.data.frame(storage_values_default(), check.names = FALSE))

    # creation
    my_parameters <- storage_values_default()
    my_parameters$efficiencywithdrawal <- 0.5
    my_parameters$`penalize-variation-injection` <- TRUE
    my_parameters$`penalize-variation-withdrawal` <- TRUE

    createClusterST(area = "fr",
                    cluster_name = "test_storage",
                    group = "new_properties",
                    storage_parameters = my_parameters,
                    overwrite = TRUE)

    createClusterST(area = "it",
                    cluster_name = "test_storage",
                    group = "new_properties",
                    storage_parameters = my_parameters,
                    overwrite = TRUE)

    # read cluster properties
    tab <- readClusterSTDesc()
    rmarkdown::paged_table(tab)

    # edit properties of existing st-storage cluster
    my_parameters$efficiencywithdrawal <- 0.9
    my_parameters$`penalize-variation-injection` <- FALSE
    my_parameters$`penalize-variation-withdrawal` <- FALSE

    editClusterST(area = "fr",
                  cluster_name = "test_storage",
                  storage_parameters = my_parameters)

    # read cluster properties
    tab <- readClusterSTDesc()
    rmarkdown::paged_table(tab)

### New optional time series

We have five new .txt files containing one series of dimension \({N=8760, P=1}\) :

- cost-injection.txt
- cost-withdrawal.txt
- cost-level.txt
- cost-variation-injection.txt
- cost-variation-withdrawal.txt

    # creation
    ratio_value <- matrix(0.7, 8760)

    # default properties with new optional TS
    createClusterST(area = "fr",
                    cluster_name = "good_ts_value",
                    cost_injection = ratio_value,
                    cost_withdrawal = ratio_value,
                    cost_level = ratio_value,
                    cost_variation_injection = ratio_value,
                    cost_variation_withdrawal = ratio_value)

    # read cluster TS values
    tab <- readInputTS(st_storage = "all",
                       showProgress = FALSE)
    rmarkdown::paged_table(head(tab))

    # edit TS values of existing st-storage cluster
    new_ratio_value <- matrix(0.85, 8760)

    # edit everything or anyone you want
    editClusterST(area = "fr",
                  cluster_name = "good_ts_value",
                  cost_injection = new_ratio_value,
                  cost_withdrawal = new_ratio_value)

    # read cluster TS values
    tab <- readInputTS(st_storage = "all",
                       showProgress = FALSE)
    rmarkdown::paged_table(head(tab))

### Additional

We can add additional constraints via the dedicated endpoints:

- constraints_properties
- TS constraints rhs_*

The function read_storages_constraints() reads all short-term storage constraints from API or disk and returns them as a nested R list. Each top-level element corresponds to an area. Inside each area you will find, for each storage cluster, two main sub-lists:

properties – general information and constraint definitions, such as:

- variable (e.g. “withdrawal”)
- operator (e.g. “equal”)
- hours (e.g. “[1, 3, 5]”)
- enabled (logical flag)

values - time-series data linked to those constraints, for example a rhs_test element containing a numeric vector of hourly values (length 8760).

#### Properties

    # Create
    createClusterST(area = "fr",
                    cluster_name = "Additional_Properties",
                    storage_parameters = my_parameters,
                    PMAX_injection = NULL,
                    PMAX_withdrawal = NULL,
                    inflows = NULL,
                    lower_rule_curve = NULL,
                    upper_rule_curve = NULL,
                    cost_injection = NULL,
                    cost_withdrawal = NULL,
                    cost_level = NULL,
                    cost_variation_injection = NULL,
                    cost_variation_withdrawal =NULL,
                    constraints_properties = list(
                      "test"=list(
                        variable = "withdrawal",
                        operator = "equal",
                        hours = c("[1,3,5]"),
                      "test2"=list(
                       variable = "netting",
                       operator = "less",
                       hours = c("[1, 168]")
                     )
                      )))

    # Edit
    editClusterST (area = "fr",
                   cluster_name = "Additional_Properties",
                   storage_parameters = my_parameters,
                    PMAX_injection = NULL,
                    PMAX_withdrawal = NULL,
                    inflows = NULL,
                    lower_rule_curve = NULL,
                    upper_rule_curve = NULL,
                    cost_injection = NULL,
                    cost_withdrawal = NULL,
                    cost_level = NULL,
                    cost_variation_injection = NULL,
                    cost_variation_withdrawal =NULL,
                   constraints_properties <- list(
                     "test"=list(
                       variable = "withdrawal",
                       operator = "equal",
                       hours = c("[1,3,5]",
                                  "[120,121,122,123,124,125,126,127,128]"),
                       enabled = FALSE
                     ),
                     "test2"=list(
                       variable = "netting",
                       operator = "less",
                       hours = c("[1, 168]")
                     )))

#### Values

    # Create
    good_ts <- matrix(0.7, nrow = 8760, ncol = 1)
    createClusterST(area = "fr",
                    cluster_name = "Additional_Values",
                    storage_parameters = my_parameters,
                    PMAX_injection = NULL,
                    PMAX_withdrawal = NULL,
                    inflows = NULL,
                    lower_rule_curve = NULL,
                    upper_rule_curve = NULL,
                    cost_injection = NULL,
                    cost_withdrawal = NULL,
                    cost_level = NULL,
                    cost_variation_injection = NULL,
                    cost_variation_withdrawal =NULL,
                    constraints_properties = list(
                      "test"=list(
                        variable = "withdrawal",
                        operator = "equal",
                        hours = c("[1,3,5]",
                                  "[120,121,122,123,124,125,126,127,128]")
                        #enabled = FALSE
                      ),
                      "test2"=list(
                        variable = "netting",
                        operator = "less",
                        hours = c("[1, 168]")
                      )),
                    # constraints_ts
                    constraints_ts = list(
                      "test" = good_ts,
                      "test2"    = good_ts
                    ))

    # Edit
    editClusterST (area = "fr",
                    cluster_name = "Additional_Values",
                   constraints_ts = list(
                     "test" = good_ts,
                     "test2"    = good_ts+1
                   )  ,
                   add_prefix = TRUE)
    #Read
    res=read_storages_constraints()

    #>                           levelName
    #> 1  Root
    #> 2   °--fr
    #> 3       ¦--fr_additional_properties
    #> 4       ¦   ¦--properties
    #> 5       ¦   ¦   °--test
    #> 6       ¦   °--values
    #> 7       °--fr_additional_values
    #> 8           ¦--properties
    #> 9           ¦   ¦--test
    #> 10          ¦   °--test2
    #> 11          °--values
    #> 12              ¦--rhs_test
    #> 13              °--rhs_test2

### Remove clusters

Nothing has changed to remove clusters.

    # read cluster names
    levels(readClusterSTDesc()$cluster)
    #> [1] "fr_additional_properties" "fr_additional_values"
    #> [3] "fr_good_ts_value"         "fr_test_storage"
    #> [5] "it_test_storage"

    # remove a cluster
    removeClusterST(area = "fr",
                    cluster_name = "good_ts_value")

    # read cluster
    tab <- readClusterSTDesc()
    rmarkdown::paged_table(tab)

## Generaldata

The “generaldata.ini” settings file (settings/generaldata.ini) contains several sections.

Antares Simulator v9.2 deletes some parameters:

- adequacy patch/enable-first-step
- adequacy patch/set-to-null-ntc-between-physical-out-for-first-step
- other preferences/initial-reservoir-levels

A message is displayed and parameters are set to `NULL` for the `[adequacy patch]` section.

For the `[other preferences]` section, the `initial-reservoir-levels` parameter is not explicitly used by a dedicated function.

    # user messages
    updateAdequacySettings(
        set_to_null_ntc_between_physical_out_for_first_step = FALSE)
    #> Warning: The `set_to_null_ntc_between_physical_out_for_first_step` argument of
    #> `updateAdequacySettings()` is deprecated as of antaresEditObject 2.9.2.
    #> ℹ This parameter are no longer supported for an Antares version >= '9.2', the
    #>   values will be ignored.
    #> This warning is displayed once every 8 hours.
    #> Call `lifecycle::last_lifecycle_warnings()` to see where this warning was
    #> generated.
    updateAdequacySettings(enable_first_step = FALSE)
    #> Warning: The `enable_first_step` argument of `updateAdequacySettings()` is deprecated as
    #> of antaresEditObject 2.9.2.
    #> ℹ This parameter are no longer supported for an Antares version >= '9.2', the
    #>   values will be ignored.
    #> This warning is displayed once every 8 hours.
    #> Call `lifecycle::last_lifecycle_warnings()` to see where this warning was
    #> generated.

## Scenario builder

The scenario builder allows you to use a new code `hfl` for ‘hydro final level’. This new feature is similar to `hl` (‘hydro levels’) and is used in the same way with the ‘coef_hydro_levels’ parameter.

    # the number of coeff is equivalent to the number of areas
      my_coef <- runif(length(getAreas()))

      opts <- simOptions()

      # build data
      ldata <- scenarioBuilder(
        n_scenario = 10,
        n_mc = 10,
        areas = getAreas(),
        coef_hydro_levels = my_coef
      )
    #> Warning: Specified number of Monte-Carlo years differ from the one in Antares
    #> general parameter

      # update scenearionbuilder.dat
      updateScenarioBuilder(ldata = ldata,
                            series = "hfl")

      readScenarioBuilder(as_matrix = TRUE)
    #> $hfl
    #>         [,1]
    #> fr 0.3920503
    #> it 0.3070450