# Diagnostics, Reliability and Predictive Maintenance of Pipeline Systems

## Documentation for package ‘pipenostics’ version 0.2.0

- DESCRIPTION file.
- Package NEWS.

## Help Pages

pipenostics-package | pipenostics: Diagnostics, Reliability and Predictive Maintenance of Pipeline Systems
api5l3t | API 5L. Values of SMYS and UTS
b31crvl | ASME B31G. Basic computer program CRVL.BAS
b31gacd | ASME B31G. Allowable corrosion depth in pipe
b31gacl | ASME B31G. Allowable corrosion length in pipe
b31gafr | ASME B31G. A-factor
b31gdata | ASME B31G. Corrosion state of 12 pipes
b31gdep | ASME B31G. Design pressure of pipe
b31gmodpf | ASME B31G. Failure pressure of the corroded pipe (modified)
b31gops | ASME B31G. Operational status of pipe
b31gpf | ASME B31G. Failure pressure of the corroded pipe (original)
b31gsap | ASME B31G. Safe maximum pressure for the corroded area of pipe
c_f | Convert to Celsius scale
c_k | Convert to Celsius scale
dnvpf | DNV-RP-F101. Failure pressure of the corroded pipe
dropg | Flow rate drop in pipe
dropp | Pressure drop in pipe
dropt | Temperature drop in cylindrical steel pipe due heat loss
flowls | List all possible flow paths in district heating network
flux_loss | Convert heat flux to specific heat loss power
fric_buzelli | Estimate pipe friction factor with Buzelli formula
fric_romeo | Estimate pipe friction factor with Romeo's formula
fric_vatankhan | Estimate pipe friction factor with Vatankhah formula
f_c | Convert to Fahrenheit scale
f_k | Convert to Fahrenheit scale
geoarea | Calculate geographical metrics
geodist | Calculate geographical metrics
inch_mm | Millimeters to inches
kgf_mpa | Megapascals to kilogram-force per square
k_c | Covert to Kelvin scale
k_f | Covert to Kelvin scale
loss_flux | Convert heat flux to specific heat loss power
m278hlair | Minenergo-278. Normative heat loss of open-air pipe
m278hlcha | Minenergo-278. Normative heat loss of pipe in channel
m278hlund | Minenergo-278. Normative heat loss of underground pipe
m278insdata | Minenergo-278. Thermal conductivity terms of pipe insulation materials
m278inshcm | Minenergo-278. Thermal conductivity of pipe insulation materials
m278soildata | Minenergo-278. Thermal conductivity of subsoil surrounding pipe
m325beta | Minenergo-325. Local heat loss coefficient
m325nhl | Minenergo-325. Normative heat loss of pipe
m325nhldata | Minenergo-325. Normative heat loss data
m325testbench | Minenergo-325. Test bench of district heating network
m325tracebw | Minenergo-325. Massively trace backwards thermal-hydraulic regime for district heating network
m325tracefw | Minenergo-325. Massively trace forwards thermal-hydraulic regime for district heating network
m325traceline | Minenergo-325. Trace thermal-hydraulic regime for linear segment of district heating network
mepof | Probability of failure of the corroded pipe within maximum entropy
meteos | Get list of weather stations (meteos)
mgtdhgeo | Get ground temperature
mgtdhgeot | Get ground temperature
mgtdhid | Get ground temperature
mgtdhidt | Get ground temperature
mm_inch | Inches to mm
mpa_kgf | Kilogram-force per square cm to megapascals
mpa_psi | Pounds per square inch to megapascals
pcorrcpf | PCORRC. Failure pressure of the corroded pipe
pipenostics | pipenostics: Diagnostics, Reliability and Predictive Maintenance of Pipeline Systems
psi_mpa | Megapascals to pounds per square inch
re_m | Estimate Reynolds number
re_u | Estimate Reynolds number
re_v | Estimate Reynolds number
shell92pf | Shell92. Failure pressure of the corroded pipe
strderate | DNV-RP-F101. De-rate yield stress and tensile strength of pipe due to temperature
tracebw | Massively trace backwards thermal-hydraulic regime for district heating network
tracefw | Massively trace forwards thermal-hydraulic regime for district heating network
traceline | Trace thermal-hydraulic regime for linear segment of district heating network
wth_d | Derive the wall thickness depending on the outside diameter of pipe